IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Time stamp: "2022-06-13T16:07:50"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.21.45 - Exporter 21.1.21.45 - Interface utilisateur alternative 21.1.21.45"
Application: "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)"

People and organizations
  Person "bjean@bimandco.com" of Organization (no name given)
  Owner history of Person "bjean@bimandco.com" of Organization (no name given) | application "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)" | change NOCHANGE | created 1655129270 (2022-06-13T14:07:50Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | object type "Niveau:Niveau 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400:RAS-2.5WHVRP1" | object type "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400:RAS-2.5WHVRP1" | names: "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400:RAS-2.5WHVRP1:16682" | material: constituents "MaterialConstituentSet" ("Aluminium": "Aluminium", "Metal": "Metal") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Autre, Contraintes, Cotes

Types
  IFCBUILDINGELEMENTPROXYTYPE "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400:RAS-2.5WHVRP1" | 1 occurrence | material: materials ("Metal", "Aluminium") | property sets: Autre, Construction, Contraintes, Cotes, Données, Données d'identification

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Catégorie = "Informations sur le projet" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Famille = "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400: RAS-2.5WHVRP1" (IFCLABEL)
    Famille et type = "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400: RAS-2.5WHVRP1" (IFCLABEL)
    ID du type = "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400: RAS-2.5WHVRP1" (IFCLABEL)
    Type = "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400: RAS-2.5WHVRP1" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Niveau 1" (IFCLABEL)
    Famille et type = "Niveau: Niveau 1" (IFCLABEL)
    ID du type = "Niveau: Niveau 1" (IFCLABEL)
    Type = "Niveau: Niveau 1" (IFCLABEL)
  Autre | properties | on 1 type object
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    MasterFormat = "Water-Source Unitary Heat Pumps" (IFCTEXT)
    Masterformat Code = "23 81 46" (IFCTEXT)
    Name BIM&CO = "Heat Pumps" (IFCTEXT)
    Nom de la famille = "Yutaki-Outdoor-Unit-R32-RAS-2.5WHVRP1_LOD400" (IFCTEXT)
    OMNICLASS Table 23 Code = "23-33 25 00" (IFCTEXT)
    Omniclass = "Air Handling Units" (IFCTEXT)
    Uniformat = "Distribution Systems" (IFCTEXT)
    Uniformat code = "D3040" (IFCTEXT)
    Working range (DHW) (°C) = "-20~35" (IFCTEXT)
    Working range (cooling) (°C) = "10~46" (IFCTEXT)
    Working range (heating) (°C) = "-20~25" (IFCTEXT)
  Graphismes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 0 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Plein" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RAS-2.5WHVRP1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RAS-2.5WHVRP1" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hitachi" (IFCLABEL)
  Contraintes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Décalage par rapport à l'hôte = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Hôte = "Niveau : Niveau 1" (IFCTEXT)
    Niveau = "Niveau: Niveau 1" (IFCLABEL)
    Élévation par rapport au niveau = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 type object
    Elévation par défaut = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Surface = 2.84729389858211 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.591453700581381 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 type object
    Height difference between OU & IU (higher OU) = 30000. (IFCLENGTHMEASURE) [MILLI METRE]
    Height difference between OU & IU (lower OU) = 20000. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum chargless piping length = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum piping length (additional refrigerant needed) = "50.00 m" (IFCTEXT)
    Miminum piping length = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Depth = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 629. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 898. (IFCLENGTHMEASURE) [MILLI METRE]
    Piping diameter (gas) ≤ 30 = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Piping diameter (gas) ≥ 30 = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Piping diameter (liquid) ≤ 30 = 6.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Piping diameter (liquid) ≥30 = 9.52 (IFCLENGTHMEASURE) [MILLI METRE]
    Refrigerant pipes connection - gas pipe diameter = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Refrigerant pipes connection - liquid pipe diameter = 9.52 (IFCLENGTHMEASURE) [MILLI METRE]
  Données d'identification | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Identifiant = "2" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 1" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 1 type object
    BC_MODEL_ID = "" (IFCTEXT)
    BC_OBJECT_ID = "215293" (IFCTEXT)
    BC_OBJECT_VERSION = "#7" (IFCTEXT)
    BC_VARIANT_ID = "562002" (IFCTEXT)
    Code d'assemblage = "" (IFCTEXT)
    Commentaires du type = "Yutaki 2.5HP outdoor unit (R32)" (IFCTEXT)
    Description = "Yutaki 2.5HP outdoor unit (R32)" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    ErP website = "https://www.hitachiaircon-erpactive.com/en/" (IFCTEXT)
    Fabricant = "Hitachi" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Keyrmark website = "" (IFCTEXT)
    Manufacturer Product Link = "" (IFCTEXT)
    Modèle = "Yutaki 2HP outdoor unit (R32) - RAS-2.5WHVRP1" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "RAS-2.5WHVRP1" (IFCTEXT)
    Numéro OmniClass = "23.75.70.17" (IFCTEXT)
    Object type = "" (IFCTEXT)
    Product Code = "RAS-2.5WHVRP1" (IFCTEXT)
    Reference = "RAS-2.5WHVRP1" (IFCTEXT)
    Titre OmniClass = "Water Heated and Cooled Terminal Heating and Cooling Units" (IFCTEXT)
  Electricité - Charges | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Numero de circuit = "" (IFCTEXT)
    Panneau = "" (IFCTEXT)
  Génie climatique | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Classification du système = "Puissance,Alimentation hydraulique" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Génie climatique | properties | on 1 type object
    Classification = "Aucun" (IFCIDENTIFIER)
  Phase de construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Visibilité | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Visi Maintenance-Installation Area = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Niveau 1" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Autre(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Contraintes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Données d'identification(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Niveau 1" (IFCTEXT)
  Construction | properties | on 1 type object
    Net Weight = 44. (IFCMASSMEASURE) [KILO GRAM]
  Données | properties | on 1 type object
    Actuator cables = "2 x 0,75mm² + GND" (IFCTEXT)
    Additional refrigerant charge needed per meter = "15 g/m" (IFCTEXT)
    Power supply cables = "2 x 4,0 mm² +GND" (IFCTEXT)
    Sound power OU = 54. (IFCREAL)
    Transmitting cables = "2 x 0,75mm² (*Shielded cable)" (IFCTEXT)
  Electricité | properties | on 1 type object
    Zmax (Ω) = 0.4 (IFCREAL)
  Electrotechnique | properties | on 1 type object
    Applicable voltage - Umax = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Applicable voltage - Umin = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    CB = 20. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    ELB = "2/40/30" (IFCTEXT)
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    MC = 17. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Maximum Current = 12.9 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Phases = 1. (IFCREAL)
  Matériaux et finitions | properties | on 1 type object
    MATERIAL = "Metal" (IFCLABEL)
  Propriétés Green Building | properties | on 1 type object
    Global Warming Potential (GWP) (kg CO2 equi/UF) = 675. (IFCREAL)
    Refrigerant Type = "R32" (IFCTEXT)
    Refrigerant charge before shipment = 1.3 (IFCMASSMEASURE) [KILO GRAM]