IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Time stamp: "2022-06-13T15:55:27"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.21.45 - Exporter 21.1.21.45 - Interface utilisateur alternative 21.1.21.45"
Application: "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)"

People and organizations
  Person "bjean@bimandco.com" of Organization (no name given)
  Owner history of Person "bjean@bimandco.com" of Organization (no name given) | application "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)" | change NOCHANGE | created 1655128527 (2022-06-13T13:55:27Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | object type "Niveau:Niveau 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400:RWD-2.5RW1E-220S" | object type "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400:RWD-2.5RW1E-220S" | names: "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400:RWD-2.5RW1E-220S:6229" | material: constituents "MaterialConstituentSet" ("CALC_HIT Logo": "CALC_HIT Logo", "CALC_Plastique blanc": "CALC_Plastique blanc", "CALC_Métal gris": "CALC_Métal gris", "CALC_Métal noir": "CALC_Métal noir", "CALC_Métal blanc": "CALC_Métal blanc") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Autre, Contraintes, Cotes

Types
  IFCBUILDINGELEMENTPROXYTYPE "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400:RWD-2.5RW1E-220S" | 1 occurrence | material: "CALC_HIT Logo" | property sets: Autre, Contraintes, Cotes, Données, Données d'identification, Electrotechnique

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Catégorie = "Informations sur le projet" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Famille = "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400: RWD-2.5RW1E-220S" (IFCLABEL)
    Famille et type = "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400: RWD-2.5RW1E-220S" (IFCLABEL)
    ID du type = "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400: RWD-2.5RW1E-220S" (IFCLABEL)
    Type = "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400: RWD-2.5RW1E-220S" (IFCLABEL)
    Visibility Maintenance-Installation Area = FALSE (IFCBOOLEAN)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Niveau 1" (IFCLABEL)
    Famille et type = "Niveau: Niveau 1" (IFCLABEL)
    ID du type = "Niveau: Niveau 1" (IFCLABEL)
    Type = "Niveau: Niveau 1" (IFCLABEL)
  Autre | properties | on 1 type object
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Name BIM&CO = "Heat Pumps" (IFCTEXT)
    Nom de la famille = "Yutaki-Indoor-Unit-SC-2-5HP-220L_LOD400" (IFCTEXT)
  Graphismes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 0 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Plein" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "RWD-2.5RW1E-220S" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RWD-2.5RW1E-220S" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCLABEL)
  Contraintes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Décalage par rapport à l'hôte = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Hôte = "Niveau : Niveau 1" (IFCTEXT)
    Niveau = "Niveau: Niveau 1" (IFCLABEL)
    Élévation par rapport au niveau = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 type object
    CALC_Offset_Depth_Gas = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_Offset_Width_Gas = 307. (IFCLENGTHMEASURE) [MILLI METRE]
    Elévation par défaut = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Surface = 7.64191787853111 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.643658503144492 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 type object
    Overall Depth = 598. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 1889. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 595. (IFCLENGTHMEASURE) [MILLI METRE]
  Données d'identification | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Identifiant = "1" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 1" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 1 type object
    Application = "Heating, Cooling, DHW with integrated tank" (IFCTEXT)
    BC_MODEL_ID = "" (IFCTEXT)
    BC_OBJECT_ID = "215302" (IFCTEXT)
    BC_OBJECT_VERSION = "#7" (IFCTEXT)
    BC_VARIANT_ID = "562076" (IFCTEXT)
    Code d'assemblage = "" (IFCTEXT)
    Commentaires du type = "Yutaki SC 2.5HP 220L indoor unit (R32)" (IFCTEXT)
    Description = "Yutaki SC 2.5HP 220L indoor unit (R32)" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Heat Pump Type = "Air-to-Water heat pump" (IFCTEXT)
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCTEXT)
    MasterFormat = "Water-Source Unitary Heat Pumps" (IFCTEXT)
    Masterformat Code = "23 81 46" (IFCTEXT)
    Modèle = "Yutaki SC 2.5HP 220L indoor unit (R32)" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "RWD-2.5RW1E-220S" (IFCTEXT)
    Numéro OmniClass = "23.75.10.00" (IFCTEXT)
    OMNICLASS Table 23 Code = "23-33 25 00" (IFCTEXT)
    Omniclass = "Air Handling Units" (IFCTEXT)
    Product Code = "RWD-2.5RW1E-220S" (IFCTEXT)
    Reference = "RWD-2.5RW1E-220S" (IFCTEXT)
    Titre OmniClass = "Transformation and Conversion of Energy" (IFCTEXT)
    Uniformat = "Distribution Systems" (IFCTEXT)
    Uniformat code = "D3040" (IFCTEXT)
  Electricité - Charges | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Numero de circuit = "" (IFCTEXT)
    Panneau = "" (IFCTEXT)
  Génie climatique | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Classification du système = "Alimentation hydraulique,Puissance,Sanitaire" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Génie climatique | properties | on 1 type object
    COP (A7/W35) = 4.8 (IFCREAL)
    COP DHW = "3.2" (IFCTEXT)
    Classification = "Aucun" (IFCIDENTIFIER)
    EER (A35/W18) = 5.3 (IFCREAL)
    EER (A35/W7) = 3.6 (IFCREAL)
    Expansion vessel - internal water volume = 0.006 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Maximum cooling capacity (A35/W18) = 7700. (IFCPOWERMEASURE) [WATT]
    Maximum cooling capacity (A35/W7) = 6000. (IFCPOWERMEASURE) [WATT]
    Maximum heating capacity (A-7/W35) = 6200. (IFCPOWERMEASURE) [WATT]
    Maximum heating capacity (A-7/W55) = 5000. (IFCPOWERMEASURE) [WATT]
    Maximum water volume at 40 °C = 0.288 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Nominal Water Flow = 0.0101039185342037 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Nominal cooling capacity (A35/W18) = 6300. (IFCPOWERMEASURE) [WATT]
    Nominal cooling capacity (A35/W7) = 5300. (IFCPOWERMEASURE) [WATT]
    Nominal energy efficiency 35°C (ηS) = 1.77 (IFCREAL)
    Nominal energy efficiency 55°C (ηS) = 1.27 (IFCREAL)
    Nominal heating capacity (A7/W35) = 6000. (IFCPOWERMEASURE) [WATT]
    Outlet water temperature (Cooling) = "5~22 °C" (IFCTEXT)
    Outlet water temperature (Heating) = "20~60 °C" (IFCTEXT)
    Reference hot water temperature = 52.85 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Standby power input DHW = 30. (IFCPOWERMEASURE) [WATT]
  Phase de construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Niveau 1" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Autre(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Contraintes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Données d'identification(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Niveau 1" (IFCTEXT)
  Données | properties | on 1 type object
    Annual energy consumption (QHE) 35°C application = 9547200000. (IFCREAL)
    Annual energy consumption (QHE) 55°C application = 11469600000. (IFCREAL)
    Energy efficiency (ηwh) = 1.3 (IFCREAL)
    Heat up time DHW = 5580. (IFCREAL)
    Load Profile DHW = "L" (IFCTEXT)
    SCOP 35°C (Average conditions) = 4.5 (IFCREAL)
    SCOP 55°C (Average conditions) = 3.24 (IFCREAL)
    SEER (+18°C / +23°C) = 8.5 (IFCREAL)
    Sound power IU = 37. (IFCREAL)
    Standby power (PSB) (Average climate) = 12. (IFCPOWERMEASURE) [WATT]
  Electrotechnique | properties | on 1 type object
    Electric heater capacity (space heating) = 3000. (IFCPOWERMEASURE) [WATT]
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Phases = 1. (IFCREAL)
    Number of poles = 1 (IFCINTEGER)