IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Time stamp: "2022-06-13T16:28:49"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.21.45 - Exporter 21.1.21.45 - Interface utilisateur alternative 21.1.21.45"
Application: "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)"

People and organizations
  Person "bjean@bimandco.com" of Organization (no name given)
  Owner history of Person "bjean@bimandco.com" of Organization (no name given) | application "Autodesk Revit 2021 (FRA)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (FRA)" | change NOCHANGE | created 1655130529 (2022-06-13T14:28:49Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | object type "Niveau:Niveau 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Yutampo II - TAW 270RHC:TAW-270RHC" | object type "Yutampo II - TAW 270RHC:TAW-270RHC" | names: "Yutampo II - TAW 270RHC:TAW-270RHC:3764" | material: constituents "MaterialConstituentSet" ("HITACHI_BLACK": "HITACHI_BLACK", "HITACHI_WHITE": "HITACHI_WHITE", "HITACHI_BLUE": "HITACHI_BLUE", "HITACHI_GREY": "HITACHI_GREY") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Pset_ManufacturerTypeInformation, Autre, Contraintes, Cotes

Types
  IFCBUILDINGELEMENTPROXYTYPE "Yutampo II - TAW 270RHC:TAW-270RHC" | 1 occurrence | material: constituents "MaterialConstituentSet" ("HITACHI_BLACK": "HITACHI_BLACK", "HITACHI_WHITE": "HITACHI_WHITE", "HITACHI_BLUE": "HITACHI_BLUE", "HITACHI_GREY": "HITACHI_GREY") | property sets: Autre, Contraintes, Cotes, Données d'identification, Electrotechnique, Génie climatique

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Catégorie = "Informations sur le projet" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Clearance Zone = FALSE (IFCBOOLEAN)
    Famille = "Yutampo II - TAW 270RHC: TAW-270RHC" (IFCLABEL)
    Famille et type = "Yutampo II - TAW 270RHC: TAW-270RHC" (IFCLABEL)
    ID du type = "Yutampo II - TAW 270RHC: TAW-270RHC" (IFCLABEL)
    Type = "Yutampo II - TAW 270RHC: TAW-270RHC" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Niveau 1" (IFCLABEL)
    Famille et type = "Niveau: Niveau 1" (IFCLABEL)
    ID du type = "Niveau: Niveau 1" (IFCLABEL)
    Type = "Niveau: Niveau 1" (IFCLABEL)
  Autre | properties | on 1 type object
    COP DHW = "3.2" (IFCTEXT)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Energy efficiency η (Average climate) = 1.29 (IFCREAL)
    Energy efficiency η (Cold climate) = 113. (IFCREAL)
    Energy efficiency η (Warm climate) = 1.4 (IFCREAL)
    Heat Pump Type = "heat pump water heater" (IFCTEXT)
    Heat up time DHW = 12600. (IFCREAL)
    Load Profile DHW = "XL" (IFCTEXT)
    MasterFormat = "Water-Source Unitary Heat Pumps" (IFCTEXT)
    Masterformat Code = "23 81 46" (IFCTEXT)
    Maximum Water Temperature = 75. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Maximum water volume at 40 °C = 0.36 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Name BIM&CO = "Heat Pumps" (IFCTEXT)
    Nom de la famille = "Yutampo II - TAW 270RHC" (IFCTEXT)
    Nominal Heating Capacity = 0. (IFCPOWERMEASURE) [WATT]
    OMNICLASS Table 23 Code = "23-33 25 00" (IFCTEXT)
    Omniclass = "Air Handling Units" (IFCTEXT)
    Reference hot water temperature = 52.8 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Refrigerant Type = "" (IFCTEXT)
    Standby power input DHW = 23. (IFCPOWERMEASURE) [WATT]
    Uniformat = "Distribution Systems" (IFCTEXT)
    Uniformat code = "D3040" (IFCTEXT)
    Working range (DHW) = "5~30" (IFCTEXT)
  Graphismes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 0 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Plein" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "TAW-270RHC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "TAW-270RHC" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCLABEL)
  Contraintes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Décalage par rapport à l'hôte = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Hôte = "Niveau : Niveau 1" (IFCTEXT)
    Niveau = "Niveau: Niveau 1" (IFCLABEL)
    Élévation par rapport au niveau = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 type object
    Elévation par défaut = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Surface = 6.97688152894082 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.482167149505645 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 type object
    Overall Depth = 681. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 1714. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Données d'identification | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Identifiant = "1" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 1" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 1 type object
    Application - MEP = "DHW" (IFCTEXT)
    BC_MODEL_ID = "" (IFCTEXT)
    BC_OBJECT_ID = "39343" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "236920" (IFCTEXT)
    Code d'assemblage = "" (IFCTEXT)
    Commentaires du type = "Indoor Unit - Tank capacity 270L" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    Fabricant = "Hitachi Air Conditioning Europe SAS" (IFCTEXT)
    Modèle = "Yutampo R32" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "TAW-270RHC" (IFCTEXT)
    Numéro OmniClass = "23.75.10.00" (IFCTEXT)
    Reference = "TAW-270RHC" (IFCTEXT)
    Titre OmniClass = "Transformation and Conversion of Energy" (IFCTEXT)
  Génie climatique | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Classification du système = "Alimentation hydraulique,Autre" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Génie climatique | properties | on 1 type object
    Classification = "Aucun" (IFCIDENTIFIER)
    Water tank capacity = 0.27 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Phase de construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Niveau 1" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Informations sur le projet" (IFCIDENTIFIER)
  Autre(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Contraintes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Données d'identification(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Niveau 1" (IFCTEXT)
  Electrotechnique | properties | on 1 type object
    Electric heater capacity (space heating) = 1640. (IFCPOWERMEASURE) [WATT]
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    IP Protection = "X1B" (IFCTEXT)
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Phases = 1. (IFCREAL)
  Matériaux et finitions | properties | on 1 type object
    Tank material = "Stainless steel (DUPLEX)" (IFCTEXT)