IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2019-01-18T10:51:51"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.3.0.0 - Interface alternative d'export 17.3.0.0"
Application: "Autodesk Revit 2017 (FRA)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (FRA)"

People and organizations
  Person "bjean@bimandco.com" of Organization (no name given)
  Owner history of Person "bjean@bimandco.com" of Organization (no name given) | application "Autodesk Revit 2017 (FRA)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (FRA)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 48° 51′ 23.807373″ | longitude 2° 21′ 7.999076″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Niveau 0" | long name "Niveau 0" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RAS-5HVNP1E" | object type "RAS-5HVNP1E" | names: "BC_Hitachi_RAS4-10-HVNP1E_LOD400:RAS-5HVNP1E:726631" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Autre, Contraintes, Cotes, Données d'identification

Types
  IFCBUILDINGELEMENTPROXYTYPE "RAS-5HVNP1E" | 1 occurrence | property sets: Analyse d'énergie(Type), Autre(Type), Cotes(Type), Données d'identification(Type), Données(Type), Electrotechnique(Type)

Property sets
  Graphismes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 0 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Plein" (IFCLABEL)
    Symbole = "Marqueur de niveau - Cercle: Marqueur de niveau - Cercle" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Données d'identification(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Pointe 8 mm" (IFCTEXT)
  Données d'identification(Type) | properties | on 1 type object
    BC_MODEL_ID = "" (IFCTEXT)
    BC_OBJECT_ID = "9563" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "35242" (IFCTEXT)
    Code d'assemblage = "" (IFCTEXT)
    Commentaires du type = "RAS HVNP1E" (IFCTEXT)
    Description = "The CENTRIFUGE IVX solution has been created for integrate this outdoor group inside the building" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    Fabricant = "HITACHI" (IFCTEXT)
    Modèle = "Outdoor Unit - IVX Premium" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "RAS-5HVNP1E" (IFCTEXT)
    Numéro OmniClass = "23.75.00.00" (IFCTEXT)
    Product Code = "7E304021" (IFCTEXT)
    Titre OmniClass = "Climate Control (HVAC)" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "RAS-5HVNP1E" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "HITACHI" (IFCLABEL)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Adresse du projet = "Entrer l'adresse ici" (IFCTEXT)
    Catégorie = "Informations sur le projet" (IFCLABEL)
    Date de fin du projet = "Date de fin" (IFCTEXT)
    Etat du projet = "Etat du projet" (IFCTEXT)
    Nom du client = "Propriétaire" (IFCTEXT)
    Nom du projet = "Nom du projet" (IFCTEXT)
    Numéro de projet = "0001" (IFCTEXT)
  Autre | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Famille = "BC_Hitachi_RAS4-10-HVNP1E_LOD400: RAS-5HVNP1E" (IFCLABEL)
    Famille et type = "BC_Hitachi_RAS4-10-HVNP1E_LOD400: RAS-5HVNP1E" (IFCLABEL)
    ID du type = "BC_Hitachi_RAS4-10-HVNP1E_LOD400: RAS-5HVNP1E" (IFCLABEL)
    Type = "BC_Hitachi_RAS4-10-HVNP1E_LOD400: RAS-5HVNP1E" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Pointe 8 mm" (IFCLABEL)
    Famille et type = "Niveau: Pointe 8 mm" (IFCLABEL)
    ID du type = "Niveau: Pointe 8 mm" (IFCLABEL)
    Type = "Niveau: Pointe 8 mm" (IFCLABEL)
  Contraintes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Décalage = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Hôte = "Niveau : Niveau 0" (IFCTEXT)
    Niveau = "Niveau: Niveau 0" (IFCLABEL)
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Surface = 8.43599404453058 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.462953088817642 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Données d'identification | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Auteur = "" (IFCTEXT)
    Description de l'organisation = "" (IFCTEXT)
    Nom de l'organisation = "" (IFCTEXT)
    Nom du bâtiment = "" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Identifiant = "3" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 0" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Electricité - Charges | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Numéro de circuit = "" (IFCTEXT)
    Panneau = "" (IFCTEXT)
  Génie climatique | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Classification du système = "Puissance,Non défini,Sanitaire" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Phase de construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Visibilité | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Service space = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Autre(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Autre(Type) | properties | on 1 type object
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Nom de la famille = "BC_Hitachi_RAS4-10-HVNP1E_LOD400" (IFCTEXT)
    Refrigerant = "R410A" (IFCTEXT)
  Contraintes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Analyse d'énergie(Type) | properties | on 1 type object
    Cooling Capacity = 134548.880208872 (IFCREAL)
    Heating Capacity = 150694.745833936 (IFCREAL)
    Nominal cooling capacity (max) = 150694.745833936 (IFCREAL)
    Nominal cooling capacity (min) = 61354.2893752454 (IFCREAL)
    Nominal heating capacity (max) = 193750.387500775 (IFCREAL)
    Nominal heating capacity (min) = 53819.5520835486 (IFCREAL)
  Cotes(Type) | properties | on 1 type object
    Fan diameter = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Height Gas pipe = 459. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Liquid pipe = 549. (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Diameter = 9.52 (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Depth = 370. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 1380. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 950. (IFCLENGTHMEASURE) [MILLI METRE]
  Données(Type) | properties | on 1 type object
    Mass = 103. (IFCREAL)
    Refrigerant charge = 4.2 (IFCREAL)
    Sound power at rated load (dB(A)) = 66. (IFCREAL)
    Sound power dB(A) = "66" (IFCTEXT)
    Sound pressure level Night mode cooling (dB(A)) = "44" (IFCTEXT)
    Sound pressure level cooling (dB(A)) = "48" (IFCTEXT)
    Sound pressure level heating (dB(A)) = "50" (IFCTEXT)
  Electrotechnique(Type) | properties | on 1 type object
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Maximum AC Voltage = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Minimum AC Voltage = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Nominal Current = 28. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Poles = "1" (IFCTEXT)
    Recommended circuit breaker = 32. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Running current cooling = 13.8 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Running current heating = 12.9 (IFCELECTRICCURRENTMEASURE) [AMPERE]
  Génie climatique - Ecoulement(Type) | properties | on 1 type object
    Maximum Air Flow = 1.5 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Génie climatique(Type) | properties | on 1 type object
    Coefficient Of Performance (COP) = 4.55 (IFCREAL)
    Energy Efficiency Ratio (EER) = 3.81 (IFCREAL)
    Maximum Connected Capacity (%) = "120" (IFCTEXT)
    Maximum Input Power = 0. (IFCPOWERMEASURE) [WATT]
    Minimum Connected Capacity (%) = "50" (IFCTEXT)
    Nominal cooling power input = 3110. (IFCPOWERMEASURE) [WATT]
    Nominal heating power input = 2910. (IFCPOWERMEASURE) [WATT]