IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2022-04-26T17:58:37"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1650988715 (2022-04-26T15:58:35Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_Duct-MSP-RPI_LOD400:RPI-2.0FSRE" | object type "BC_Hitachi_Duct-MSP-RPI_LOD400:RPI-2.0FSRE" | names: "BC_Hitachi_Duct-MSP-RPI_LOD400:RPI-2.0FSRE:7084" | material: materials ("<Unnamed>", "HITACHI_WHITE", "HITACHI_Pink") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_Duct-MSP-RPI_LOD400:RPI-2.0FSRE" | 1 occurrence | material: materials ("<Unnamed>", "HITACHI_WHITE", "HITACHI_Pink") | property sets: Constraints, Dimensions, Electrical, Electrical Engineering, Identity Data, Mechanical

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Clearance Zone = TRUE (IFCBOOLEAN)
    Family = "BC_Hitachi_Duct-MSP-RPI_LOD400: RPI-2.0FSRE" (IFCLABEL)
    Family and Type = "BC_Hitachi_Duct-MSP-RPI_LOD400: RPI-2.0FSRE" (IFCLABEL)
    Type = "BC_Hitachi_Duct-MSP-RPI_LOD400: RPI-2.0FSRE" (IFCLABEL)
    Type Id = "BC_Hitachi_Duct-MSP-RPI_LOD400: RPI-2.0FSRE" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Acoustic Pressure Level Maxi = 32. (IFCREAL)
    Capacité de Chauffage Nominale = 6300. (IFCPOWERMEASURE) [WATT]
    Capacité de Refroidissement Nominale = 5600. (IFCPOWERMEASURE) [WATT]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "BC_Hitachi_Duct-MSP-RPI_LOD400" (IFCTEXT)
    MasterFormat = "23 73 00" (IFCTEXT)
    Niveau de pression acoustique max = 32. (IFCREAL)
    Nom OmniClass = "" (IFCTEXT)
    Nominal Cooling Capacity = 5600. (IFCPOWERMEASURE) [WATT]
    Nominal Heating Capacity = 6300. (IFCPOWERMEASURE) [WATT]
    OMNICLASS Table 23 Code = "23.75.10.00" (IFCTEXT)
    Omniclass = "23-33 25 00" (IFCTEXT)
    Puissance Acoustique Maximum = 58 (IFCINTEGER)
    Refrigerant Type = "R410A / R32" (IFCTEXT)
    Sound power max = 58 (IFCINTEGER)
    Type de réfrigérant = "R410A / R32" (IFCTEXT)
    Uniformat = "D3040" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RPI-2.0FSRE" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RPI-2.0FSRE" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    CALC_DGL = 15.9 (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_DLL = 6.4 (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_HAI = 174. (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_HAO = 162. (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_LAI = 663. (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_LAO = 524. (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_Lt1 = 97.6473078065622 (IFCLENGTHMEASURE) [MILLI METRE]
    CALC_Lt2 = 238.647307806621 (IFCLENGTHMEASURE) [MILLI METRE]
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 5.34241869319423 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.904022283800479 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Diamètre Etat Liquide = 6.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre Evacuation = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre Gaz = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de Reprise = 174. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de Soufflage = 162. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur hors tout = 240. (IFCLENGTHMEASURE) [MILLI METRE]
    Input Height = 174. (IFCLENGTHMEASURE) [MILLI METRE]
    Input Width = 663. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur de Reprise = 663. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur de Soufflage = 524. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur hors tout = 750. (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Diameter = 6.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Outlet Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Output Height = 162. (IFCLENGTHMEASURE) [MILLI METRE]
    Output Width = 524. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall depth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 240. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 750. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur hors tout = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "520228" (IFCTEXT)
    BC_OBJECT_ID = "208597" (IFCTEXT)
    BC_OBJECT_VERSION = "#4" (IFCTEXT)
    BC_VARIANT_ID = "507783" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Duct MSP (RPI-FSRE/FSN6E)" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCTEXT)
    Model = "Duct MSP (RPI-FSRE/FSN6E)" (IFCTEXT)
    Numéro d'article commerce international (NACI) = "" (IFCTEXT)
    OmniClass Number = "23.75.10.00" (IFCTEXT)
    OmniClass Title = "Transformation and Conversion of Energy" (IFCTEXT)
    Reference = "RPI-2.0FSRE" (IFCTEXT)
    Référence = "RPI-2.0FSRE" (IFCTEXT)
    Type Comments = "RPI-2.0FSRE" (IFCTEXT)
    Type Name = "RPI-2.0FSRE" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Other,Return Air,Supply Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Electrical | properties | on 1 type object
    AC Nominal Power = 150. (IFCPOWERMEASURE) [WATT]
    Current Rating = 1.4 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Current max DC = 1.8 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Effective rated output = 150. (IFCPOWERMEASURE) [WATT]
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Maximum AC Voltage = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Minimum AC Voltage = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Nominal Current = 1.4 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Poles = 1 (IFCINTEGER)
    Usage Current = 1.4 (IFCELECTRICCURRENTMEASURE) [AMPERE]
  Electrical Engineering | properties | on 1 type object
    Calibre d'Intensité = 1.4 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Courant DC Maximal = 1.8 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Courant Nominal = 1.4 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Courant d'usage = 1.4 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Fréquence = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Nombres de Pôles = 1 (IFCINTEGER)
    Puissance AC Nominale = 150. (IFCPOWERMEASURE) [WATT]
    Puissance utile nominale = 150. (IFCPOWERMEASURE) [WATT]
    Tension AC Min = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Tension AC max = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Tension Nominale = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Mechanical - Flow | properties | on 1 type object
    Capacity = 5600. (IFCPOWERMEASURE) [WATT]
    Capacité = 5600. (IFCPOWERMEASURE) [WATT]
    Chute de Pression Evacuation = 0.0015 (IFCPRESSUREMEASURE) [PASCAL]
    Débit Air Maximum = 233.333333333333 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Exhaust Pressure Drop = 0.0015 (IFCPRESSUREMEASURE) [PASCAL]
    Maximum Air Flow = 233.333333333333 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]