IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2023-05-11T10:36:20"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Default UI"
Application: "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)"

People and organizations
  Person "bjean@bimandco.com" of Organization (no name given)
  Owner history of Person "bjean@bimandco.com" of Organization (no name given) | application "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RCI-1.5FSRE" | object type "RCI-1.5FSRE" | names: "BC_Hitachi_Cassette-RCI-FSRE-1.0-6.0_LOD400:RCI-1.5FSRE:3847" | material: materials ("Steel, RQC100", "Operation space", "Service space", "Plastic, Opaque White", "Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Autre, Contraintes, Cotes, Données d'identification

Types
  IFCBUILDINGELEMENTPROXYTYPE "RCI-1.5FSRE" | 1 occurrence | material: materials ("Steel, RQC100", "Operation space", "Service space", "Plastic, Opaque White", "Copper") | property sets: Analyse d'énergie, Autre, Construction, Contraintes, Cotes, Données

Property sets
  Graphismes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 0 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Plein" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "RCI-1.5FSR" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCLABEL)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Catégorie = "Informations sur le projet" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Famille = "BC_Hitachi_Cassette-RCI-FSRE-1.0-6.0_LOD400: RCI-1.5FSRE" (IFCLABEL)
    Famille et type = "BC_Hitachi_Cassette-RCI-FSRE-1.0-6.0_LOD400: RCI-1.5FSRE" (IFCLABEL)
    ID du type = "BC_Hitachi_Cassette-RCI-FSRE-1.0-6.0_LOD400: RCI-1.5FSRE" (IFCLABEL)
    Type = "BC_Hitachi_Cassette-RCI-FSRE-1.0-6.0_LOD400: RCI-1.5FSRE" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Niveau 1" (IFCLABEL)
    Famille et type = "Niveau: Niveau 1" (IFCLABEL)
    ID du type = "Niveau: Niveau 1" (IFCLABEL)
    Type = "Niveau: Niveau 1" (IFCLABEL)
  Autre | properties | on 1 type object
    Acoustic Pressure Level Maxi = 35. (IFCREAL)
    Acoustic Pressure Level Mini = 27. (IFCREAL)
    Capacité de Chauffage Nominale = 43055.6416668389 (IFCREAL)
    Capacité de Refroidissement Nominale = 38750.077500155 (IFCREAL)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Code BIM&CO = "" (IFCTEXT)
    Code Masterformat = "23 73 00" (IFCTEXT)
    Code OMNICLASS Table 23 = "23.75.70.00" (IFCTEXT)
    Code Uniformat = "D3040" (IFCTEXT)
    Coefficient de Performance (COP) = 0. (IFCREAL)
    Description OmniClass = "Air Handling Units" (IFCTEXT)
    MasterFormat = "Indoor Central-Station Air-Handling Units" (IFCTEXT)
    Masterformat Code = "23 73 00" (IFCTEXT)
    Name BIM&CO = "Indoor Unit" (IFCTEXT)
    Niveau de pression acoustique max = 35. (IFCREAL)
    Nom BIM&CO = "HVAC" (IFCTEXT)
    Nom de la famille = "BC_Hitachi_Cassette-RCI-FSRE-1.0-6.0_LOD400" (IFCTEXT)
    Numéro OmniClass = "23-33 25 00" (IFCTEXT)
    OmniClass code = "23-33 25 00" (IFCTEXT)
    OmniClass description = "Air Handling Units" (IFCTEXT)
    Omniclass = "HVAC Distribution Devices" (IFCTEXT)
    Pression Acoustique à Vitesse minimum = 27. (IFCREAL)
    Puissance Nominale Chauffage = 0. (IFCPOWERMEASURE) [WATT]
    Puissance Nominale Froid = 0. (IFCPOWERMEASURE) [WATT]
    Puissance Sélection Chauffage = 0. (IFCPOWERMEASURE) [WATT]
    Puissance Sélection Froid = 0. (IFCPOWERMEASURE) [WATT]
    Puissance Thermique = 0. (IFCPOWERMEASURE) [WATT]
    Puissance acoustique à Pn = 53. (IFCREAL)
    Refrigerant Type = "R410A / R32" (IFCTEXT)
    Sound power at rated load = 53. (IFCREAL)
    Température Basse Sortie Eau = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Température Haute Sortie Eau = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Type de réfrigérant = "R410A / R32" (IFCTEXT)
    Uniformat = "Distribution Systems" (IFCTEXT)
    Uniformat code = "D3040" (IFCTEXT)
  Contraintes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Hôte = "Aucun(e)" (IFCTEXT)
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 type object
    Elévation par défaut = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Profondeur Service space = 257.999999999967 (IFCLENGTHMEASURE) [MILLI METRE]
    Surface = 23.0046289657802 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 4.79026913336381 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 type object
    Diamètre Etat Liquide = 6.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre Evacuation = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre Gaz = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Face Depth = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Face Height = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Face Width = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur hors tout = 840. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur hors tout = 840. (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Diameter = 6.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Longueur hors tout = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Outlet Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall depth = 248. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 840. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 840. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur hors tout = 248. (IFCLENGTHMEASURE) [MILLI METRE]
    Épaisseur hors tout = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Données d'identification | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Identifiant = "1" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 1" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 1 type object
    BC_MODEL_ID = "868599" (IFCTEXT)
    BC_OBJECT_ID = "287274" (IFCTEXT)
    BC_OBJECT_VERSION = "#9" (IFCTEXT)
    BC_VARIANT_ID = "710978" (IFCTEXT)
    Code Produit = "" (IFCTEXT)
    Code d'assemblage = "" (IFCTEXT)
    Commentaires du type = "RCI-1.5FSR" (IFCTEXT)
    Date de Création = "5/10/2023 6:03:54 PM" (IFCTEXT)
    Description = "RCI-FSRE" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    Fabricant = "Hitachi Air Conditioning Europe SAS" (IFCTEXT)
    Lien de l'Objet sur le site fabricant = "" (IFCTEXT)
    Modèle = "RCI-FSRE" (IFCTEXT)
    Nom = "RCI-FSRE" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "RCI-1.5FSRE" (IFCTEXT)
    Numéro OmniClass = "23.75.70.00" (IFCTEXT)
    Numéro d'article commerce international (NACI) = "" (IFCTEXT)
    Reference = "RCI-1.5FSR" (IFCTEXT)
    Référence = "RCI-1.5FSRE" (IFCTEXT)
    Titre OmniClass = "HVAC Distribution Devices" (IFCTEXT)
    Type de l'Objet = "Indoor Unit" (IFCTEXT)
    URL = "" (IFCTEXT)
    URL de l'Auteur = "https://www.bimandco.com/en/users/hcrmxlsmdu" (IFCTEXT)
  Génie climatique | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Classification du système = "Non défini,Sanitaire,Puissance" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Génie climatique | properties | on 1 type object
    Air Flow (HiH/Hi/Me/low) m3/min = "21 / 17 / 14 / 11" (IFCTEXT)
    Classification = "Aucun" (IFCIDENTIFIER)
    Fan motor input = 57. (IFCPOWERMEASURE) [WATT]
  Phase de construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Visibilité | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Operation space = TRUE (IFCBOOLEAN)
    Service space = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Autre(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Contraintes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Données d'identification(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Niveau 1" (IFCTEXT)
  Analyse d'énergie | properties | on 1 type object
    Cooling Capacity = 38750.077500155 (IFCREAL)
    Heating Capacity = 43055.6416668389 (IFCREAL)
  Construction | properties | on 1 type object
    Mass = 27.5 (IFCREAL)
    Masse = 27.5 (IFCREAL)
    Poids Brut = 0. (IFCREAL)
    Volume Nominal Ballon = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Données | properties | on 1 type object
    Niveau de Pression Acoustique = 0. (IFCREAL)
    Numéro de l'Etage = "" (IFCTEXT)
  Electrotechnique | properties | on 1 type object
    Calibre d'Intensité = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Calibre de disjoncteur = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Canalisations Préfabriquées de Transport = FALSE (IFCBOOLEAN)
    Charge réelle sortie phase 1 = 0. (IFCPOWERMEASURE) [WATT]
    Charge réelle sortie phase 2 = 0. (IFCPOWERMEASURE) [WATT]
    Charge réelle sortie phase 3 = 0. (IFCPOWERMEASURE) [WATT]
    Cos φ = 0. (IFCREAL)
    Couplage = "" (IFCTEXT)
    Courant AC Max = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Courant Batterie = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Courant DC Maximal = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Courant d'usage = 5. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Diamètre de l'âme = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Fréquence = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Indice Horaire = "" (IFCTEXT)
    Maximum AC Voltage = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Minimum AC Voltage = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Nombres de Pôles = 1 (IFCINTEGER)
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Poles = 1 (IFCINTEGER)
    Puissance AC Max = 0. (IFCPOWERMEASURE) [WATT]
    Puissance AC Nominale = 0. (IFCPOWERMEASURE) [WATT]
    Puissance absorbée aux conditions nominales = 0. (IFCPOWERMEASURE) [WATT]
    Puissance active de l'utilisation = 0. (IFCPOWERMEASURE) [WATT]
    Puissance frigorifique nominale = 0. (IFCPOWERMEASURE) [WATT]
    Tension AC Min = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Tension AC max = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Tension Nominale = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Tension Nominale du Circuit de Charge Batteries = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Usage Current = 5. (IFCELECTRICCURRENTMEASURE) [AMPERE]
  Génie climatique - Ecoulement | properties | on 1 type object
    CTA double étage = FALSE (IFCBOOLEAN)
    Capacité = 0. (IFCPOWERMEASURE) [WATT]
    Chute de Pression Evacuation = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Débit Air Maximum = 12.360133352521 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit Air Minimum = 6.47435556560624 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Maximum Air Flow = 12.360133352521 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Minimum Air Flow = 6.47435556560624 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Pression Maximum Air = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Matériaux et finitions | properties | on 1 type object
    Color = "Neutral white (4.56Y8.85/0.38)" (IFCTEXT)
    Couleur = "Neutral white (4.56Y8.85/0.38)" (IFCTEXT)
  Plomberie | properties | on 1 type object
    Débit nominal ECS = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]