IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2022-02-22T14:24:48"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1645536288 (2022-02-22T13:24:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400:RCI-6.0FSR" | object type "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400:RCI-6.0FSR" | names: "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400:RCI-6.0FSR:4035" | material: materials ("Steel, RQC100", "Operation space", "Service space", "Plastic, Opaque White", "Copper") | property sets: Pset_BuildingElementProxyCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400:RCI-6.0FSR" | 1 occurrence | material: "Steel, RQC100" | property sets: Constraints, Construction, Dimensions, Electrical Engineering, Energy Analysis, Identity Data

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400: RCI-6.0FSR" (IFCLABEL)
    Family and Type = "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400: RCI-6.0FSR" (IFCLABEL)
    Type = "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400: RCI-6.0FSR" (IFCLABEL)
    Type Id = "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400: RCI-6.0FSR" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Acoustic Pressure Level Maxi = 48. (IFCREAL)
    Acoustic Pressure Level Mini = 37. (IFCREAL)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "BC_Hitachi_Cassette-RCI-FSR-1.0-6.0_LOD400" (IFCTEXT)
    MasterFormat = "Indoor Central-Station Air-Handling Units" (IFCTEXT)
    Masterformat Code = "23 73 00" (IFCTEXT)
    Name BIM&CO = "Indoor Unit" (IFCTEXT)
    OmniClass code = "23-33 25 00" (IFCTEXT)
    OmniClass description = "Air Handling Units" (IFCTEXT)
    Refrigerant Type = "R410A / R32" (IFCTEXT)
    Sound power at rated load = 65. (IFCREAL)
    Uniformat = "Distribution Systems" (IFCTEXT)
    Uniformat code = "D3040" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RCI-6.0FSR" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Color = "Neutral white (4.56Y8.85/0.38)" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RCI-6.0FSR" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 23.6366848337194 (IFCAREAMEASURE) [SQUARE_METRE]
    Profondeur Service space = 257.999999999967 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 5.71638935390695 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Face Depth = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Face Height = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Face Width = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Diameter = 9.52 (IFCLENGTHMEASURE) [MILLI METRE]
    Outlet Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall depth = 298. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 840. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 840. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "514289" (IFCTEXT)
    BC_OBJECT_ID = "209116" (IFCTEXT)
    BC_OBJECT_VERSION = "" (IFCTEXT)
    BC_VARIANT_ID = "508746" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Standard Cassette 800*800.Individual control setting for each louver. Suitable up to 4,2 m height under ceiling . Optional motion sensor" (IFCTEXT)
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCTEXT)
    Model = "Cassette 800 x 800 RCI FSR" (IFCTEXT)
    OmniClass Number = "23.75.70.00" (IFCTEXT)
    OmniClass Title = "HVAC Distribution Devices" (IFCTEXT)
    Product Code = "70405309" (IFCTEXT)
    Reference = "RCI-6.0FSR" (IFCTEXT)
    Type Comments = "RCI-6.0FSR" (IFCTEXT)
    Type Name = "RCI-6.0FSR" (IFCTEXT)
    URL = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Undefined,Sanitary,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Air Flow (HiH/Hi/Me/low) m3/min = "37 / 35 / 28 / 22" (IFCTEXT)
    Classification = "None" (IFCIDENTIFIER)
    Fan motor input = 127. (IFCPOWERMEASURE) [WATT]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Operation space = TRUE (IFCBOOLEAN)
    Service space = TRUE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Mass = 32.5 (IFCMASSMEASURE) [KILO GRAM]
  Electrical Engineering | properties | on 1 type object
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Maximum AC Voltage = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Minimum AC Voltage = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Poles = 1 (IFCINTEGER)
    Tension AC max = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Usage Current = 5. (IFCELECTRICCURRENTMEASURE) [AMPERE]
  Energy Analysis | properties | on 1 type object
    Cooling Capacity = 14000. (IFCPOWERMEASURE) [WATT]
    Heating Capacity = 16000. (IFCPOWERMEASURE) [WATT]
  Materials and Finishes | properties | on 1 type object
    Color = "Neutral white (4.56Y8.85/0.38)" (IFCTEXT)
    Couleur = "Neutral white (4.56Y8.85/0.38)" (IFCTEXT)
  Mechanical - Flow | properties | on 1 type object
    Maximum Air Flow = 616.666666666666 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Minimum Air Flow = 366.666666666667 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]