IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2022-04-27T15:01:39"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20181015_0930(x64) - Exporter 18.4.0.0 - Interface alternative d'export 18.4.0.0"
Application: "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)"

People and organizations
  Person "bjean@bimandco.com" of Organization (no name given)
  Owner history of Person "bjean@bimandco.com" of Organization (no name given) | application "Autodesk Revit 2018 (FRA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (FRA)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 48° 51′ 23.999633″ | longitude 2° 21′ 3.553905″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Niveau 1" | long name "Niveau 1" | object type "Niveau:Pointe 8 mm" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RPK-0.4FSRM" | object type "BC_Hitachi_RPK-FSRHM_LOD400:RPK-0.4FSRM" | names: "BC_Hitachi_RPK-FSRHM_LOD400:RPK-0.4FSRM:137386" | material: "Color" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Autre, Contraintes, Cotes

Types
  IFCBUILDINGELEMENTPROXYTYPE "RPK-0.4FSRM" | 1 occurrence | material: "Color" | property sets: Analyse d'énergie, Autre, Construction, Contraintes, Cotes, Données

Property sets
  Graphismes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 0 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Centre" (IFCLABEL)
    Symbole = "Marqueur de niveau - Cercle: Marqueur de niveau - Cercle" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Données d'identification | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Auteur = "" (IFCTEXT)
    Description de l'organisation = "" (IFCTEXT)
    Nom de l'organisation = "" (IFCTEXT)
    Nom du bâtiment = "" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Identifiant = "1" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 1" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 1 type object
    BC_MODEL_ID = "" (IFCTEXT)
    BC_OBJECT_ID = "209117" (IFCTEXT)
    BC_OBJECT_VERSION = "#21" (IFCTEXT)
    BC_VARIANT_ID = "508755" (IFCTEXT)
    Code d'assemblage = "" (IFCTEXT)
    Commentaires du type = "RPK-0.4FSRM" (IFCTEXT)
    Description = "Wall Hung without electronic expansion valve inside" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    Fabricant = "Hitachi Air Conditioning Europe SAS" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Manufacturer Product Link = "" (IFCTEXT)
    Modèle = "Indoor unit - Wall hung RPK - FSR(H)M" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "RPK-0.4FSRM" (IFCTEXT)
    Numéro OmniClass = "23.75.00.00" (IFCTEXT)
    Product Code = "60279204" (IFCTEXT)
    Reference = "RPK-0.4FSRM" (IFCTEXT)
    Titre OmniClass = "Climate Control (HVAC)" (IFCTEXT)
  Données d'identification(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Pointe 8 mm" (IFCTEXT)
  Contraintes(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Adresse du projet = "Entrer l'adresse ici" (IFCTEXT)
    Catégorie = "Informations sur le projet" (IFCLABEL)
    Date de fin du projet = "Date de fin" (IFCTEXT)
    Etat du projet = "Etat du projet" (IFCTEXT)
    Nom du client = "Propriétaire" (IFCTEXT)
    Nom du projet = "Nom du projet" (IFCTEXT)
    Numéro de projet = "0001" (IFCTEXT)
  Autre | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    Famille = "BC_Hitachi_RPK-FSRHM_LOD400: RPK-0.4FSRM" (IFCLABEL)
    Famille et type = "BC_Hitachi_RPK-FSRHM_LOD400: RPK-0.4FSRM" (IFCLABEL)
    ID du type = "BC_Hitachi_RPK-FSRHM_LOD400: RPK-0.4FSRM" (IFCLABEL)
    Niveau de nomenclature = "Niveau: Niveau 1" (IFCLABEL)
    Type = "BC_Hitachi_RPK-FSRHM_LOD400: RPK-0.4FSRM" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Pointe 8 mm" (IFCLABEL)
    Famille et type = "Niveau: Pointe 8 mm" (IFCLABEL)
    ID du type = "Niveau: Pointe 8 mm" (IFCLABEL)
    Type = "Niveau: Pointe 8 mm" (IFCLABEL)
  Autre | properties | on 1 type object
    Catégorie = "Equipement de génie climatique" (IFCLABEL)
    MasterFormat = "Indoor Central-Station Air-Handling Units" (IFCTEXT)
    Masterformat Code = "23 73 00" (IFCTEXT)
    Name BIM&CO = "Indoor Unit" (IFCTEXT)
    Nom de la famille = "BC_Hitachi_RPK-FSRHM_LOD400" (IFCTEXT)
    OmniClass code = "23-33 25 00" (IFCTEXT)
    OmniClass description = "Air Handling Units" (IFCTEXT)
    Refrigerant Type = "R410A / R32" (IFCTEXT)
    Sound Power Min = 45 (IFCINTEGER)
    Uniformat = "Distribution Systems" (IFCTEXT)
  Autre(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RPK-0.4FSRM" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RPK-0.4FSRM" (IFCIDENTIFIER)
  Contraintes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Hôte = "Niveau : Niveau 1" (IFCTEXT)
    Niveau = "Niveau: Niveau 1" (IFCLABEL)
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Contraintes | properties | on 1 type object
    Diameter left side pipe wire hole = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Diameter right side pipe wire hole = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance Gas pipe = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance rear left side pipe wire hole = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance rear right side pipe wire hole = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Elévation par défaut = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Operation and service space - a = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Operation and service space - b = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Operation and service space - c = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Operation and service space - d = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Surface = 2.51197207452162 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0466448216517259 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Cotes | properties | on 1 type object
    Gas Diameter = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Diameter = 6.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Outlet Diameter = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall depth = 230. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall width = 790. (IFCLENGTHMEASURE) [MILLI METRE]
  Electricité - Charges | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Numéro de circuit = "" (IFCTEXT)
    Panneau = "" (IFCTEXT)
  Génie climatique | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Classification du système = "Non défini,Sanitaire,Puissance" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Génie climatique | properties | on 1 type object
    Classification = "Aucun" (IFCIDENTIFIER)
  Phase de construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase de création = "Phase 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Analyse d'énergie | properties | on 1 type object
    Cooling Capacity = 11840.3014583807 (IFCREAL)
    Heating Capacity = 13993.0835417226 (IFCREAL)
    Nominal cooling capacity (UTOPIA) = 0. (IFCREAL)
    Nominal heating capacity (UTOPIA) = 0. (IFCREAL)
  Construction | properties | on 1 type object
    Net Weight = 9. (IFCREAL)
  Données | properties | on 1 type object
    Engine Power = 40. (IFCPOWERMEASURE) [WATT]
    Packaging volume = 0.09 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Refrigerant pipe connection = "Flare nuts" (IFCTEXT)
    Remote control = "PC-ARFP1E / PC-AWR (*)" (IFCTEXT)
    Sound power level - Speed Hi2 (dB(A)) = 49. (IFCREAL)
    Sound power level - Speed Medium (dB(A)) = 46. (IFCREAL)
    Sound pressure level - Speed Hi (dB(A)) = 31. (IFCREAL)
    Sound pressure level - Speed Hi2 (dB(A)) = 32. (IFCREAL)
    Sound pressure level - Speed Low (dB(A)) = 30. (IFCREAL)
    Sound pressure level - Speed Medium (dB(A)) = 29. (IFCREAL)
  Electrotechnique | properties | on 1 type object
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Maximum Current = 5. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Génie climatique - Ecoulement | properties | on 1 type object
    Air Flow - Speed Hi = 4.29661778444778 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Air Flow - Speed Medium = 3.94347111723289 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Matériaux et finitions | properties | on 1 type object
    Operation and service space - Material = "Operation and service space" (IFCLABEL)
  Visibilité | properties | on 1 type object
    Operation and service space = FALSE (IFCBOOLEAN)

Other addresses and roles
  2 x postal address: "Entrer l'adresse ici", "Paris", "France"