IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-06-04T15:49:38"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_0715(x64) - Exporter 2015.0.2016.0512 - Default UI"
Application: "Autodesk Revit MEP 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit MEP 2015 (ENU)"

People and organizations
  Person "valentino.jugovic" of Organization (no name given)
  Owner history of Person "valentino.jugovic" of Organization (no name given) | application "Autodesk Revit MEP 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit MEP 2015 (ENU)" | change NOCHANGE | created 1559601733 (2019-06-03T22:42:13Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "MC-9-D" | names: "TopVent_MC:MC-9-D:925353" | material: materials ("HOVAL WHITE", "HOVAL RED", "HOVAL GRAY") | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Graphics, Identity Data, Mechanical

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "TopVent_MC: MC-9-D" (IFCLABEL)
    Family and Type = "TopVent_MC: MC-9-D" (IFCLABEL)
    Type = "TopVent_MC: MC-9-D" (IFCLABEL)
    Type Id = "TopVent_MC: MC-9-D" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    COBIE Air flow rate = "5000.0 m3/h" (IFCTEXT)
    COBIE Condensate quantity 28 °C (6/12 °C) = "0.0/0.1 kg/h" (IFCTEXT)
    COBIE Condensate quantity 28 °C (8/14 °C) = "0.0/0.0 kg/h" (IFCTEXT)
    COBIE Condensate quantity 32 °C (6/12 °C) = "25.6/31.2 kg/h" (IFCTEXT)
    COBIE Condensate quantity 32 °C (8/14 °C) = "15.7/21.3 kg/h" (IFCTEXT)
    COBIE Condensate quantity = "150.0 kg/h" (IFCTEXT)
    COBIE Connected load = "3.6 kW" (IFCTEXT)
    COBIE Current consumption max. = "5.9A" (IFCTEXT)
    COBIE Effective electric power input = "1.56 kW" (IFCTEXT)
    COBIE Extract air temperature max. = "50°C" (IFCTEXT)
    COBIE Floor area covered = "946.0" (IFCTEXT)
    COBIE Frequency = "50 Hz" (IFCTEXT)
    COBIE Heat output -5/-15 °C (60/40 °C) = "86.7/89.3 kW" (IFCTEXT)
    COBIE Heat output -5/-15 °C (80/60 °C) = "142.0/144.6 kW" (IFCTEXT)
    COBIE Maximum mounting height -5/-15 °C (60/40 °C) = "11.7/11.7 m" (IFCTEXT)
    COBIE Maximum mounting height -5/-15 °C (80/60 °C) = "9.3/9.4 m" (IFCTEXT)
    COBIE Nominal air flow rate = "9000.0" (IFCTEXT)
    COBIE Octave sound power level - 1000 Hz = "75 dB" (IFCTEXT)
    COBIE Octave sound power level - 125 Hz = "67 dB" (IFCTEXT)
    COBIE Octave sound power level - 2000 Hz = "75 dB" (IFCTEXT)
    COBIE Octave sound power level - 250 Hz = "70 dB" (IFCTEXT)
    COBIE Octave sound power level - 4000 Hz = "74 dB" (IFCTEXT)
    COBIE Octave sound power level - 500 Hz = "73 dB" (IFCTEXT)
    COBIE Octave sound power level - 63 Hz = "49 dB" (IFCTEXT)
    COBIE Octave sound power level - 8000 Hz = "68 dB" (IFCTEXT)
    COBIE Permitted voltage tolerance = "+/-5%" (IFCTEXT)
    COBIE Pressure of the heating medium max. = "800 kPa" (IFCTEXT)
    COBIE Protection rating = "IP 54" (IFCTEXT)
    COBIE Relative humidity of the fresh air 28 °C (6/12 °C) = "40/60 %" (IFCTEXT)
    COBIE Relative humidity of the fresh air 32 °C (6/12 °C) = "40/60 %" (IFCTEXT)
    COBIE Sensible cooling capacity 28 °C (6/12 °C) = "38.1/37.7 kW" (IFCTEXT)
    COBIE Sensible cooling capacity 28 °C (8/14 °C) = "33.2/32.9 kW" (IFCTEXT)
    COBIE Sensible cooling capacity 32 °C (6/12 °C) = "47.4/47.1 kW" (IFCTEXT)
    COBIE Sensible cooling capacity 32 °C (8/14 °C) = "42.6/42.2 kW" (IFCTEXT)
    COBIE Series fuse = "13A" (IFCTEXT)
    COBIE Sound pressure level (at a distance of 5 m) = "59 dB(A)" (IFCTEXT)
    COBIE Static efficiency of the fans = "63.6%" (IFCTEXT)
    COBIE Supply air temperature -5/-15 °C (60/40 °C) = "46.1/46.0 °C" (IFCTEXT)
    COBIE Supply air temperature -5/-15 °C (80/60 °C) = "64.4/64.2 °C" (IFCTEXT)
    COBIE Supply air temperature 28 °C (6/12 °C) = "11.8/12.0 kW" (IFCTEXT)
    COBIE Supply air temperature 28 °C (8/14 °C) = "13.4/13.6 °C" (IFCTEXT)
    COBIE Supply air temperature 32 °C (6/12 °C) = "12.7/12.9 kW" (IFCTEXT)
    COBIE Supply air temperature 32 °C (8/14 °C) = "14.3/14.5 °C" (IFCTEXT)
    COBIE Supply air temperature max. = "60°C" (IFCTEXT)
    COBIE Supply voltage = "3x400 V AC" (IFCTEXT)
    COBIE Temperature of the heating medium max. = "90°C" (IFCTEXT)
    COBIE Total cooling capacity 28 °C (6/12 °C) = "38.1/37.8 kW" (IFCTEXT)
    COBIE Total cooling capacity 28 °C (8/14 °C) = "33.2/32.9 kW" (IFCTEXT)
    COBIE Total cooling capacity 32 °C (6/12 °C) = "64.8/68.3 kW" (IFCTEXT)
    COBIE Total cooling capacity 32 °C (8/14 °C) = "53.3/56.7 kW" (IFCTEXT)
    COBIE Total sound power level = "81 dB(A)" (IFCTEXT)
    COBIE Water content of heating coil = "7.9 l" (IFCTEXT)
    COBIE Water pressure drop -5/-15 °C (60/40 °C) = "6/6 kPa" (IFCTEXT)
    COBIE Water pressure drop -5/-15 °C (80/60 °C) = "15/15 kPa" (IFCTEXT)
    COBIE Water pressure drop 28 °C (6/12 °C) = "13/13 kW" (IFCTEXT)
    COBIE Water pressure drop 28 °C (8/14 °C) = "10/10 kPa" (IFCTEXT)
    COBIE Water pressure drop 32 °C (6/12 °C) = "39/43 kW" (IFCTEXT)
    COBIE Water pressure drop 32 °C (8/14 °C) = "26/30 kPa" (IFCTEXT)
    COBIE Water quantity -5/-15 °C (60/40 °C) = "3725/3837 l/h" (IFCTEXT)
    COBIE Water quantity -5/-15 °C (80/60 °C) = "6101/6212 l/h" (IFCTEXT)
    COBIE Water quantity 28 °C (6/12 °C) = "5451/5409 l/h" (IFCTEXT)
    COBIE Water quantity 28 °C (8/14 °C) = "4756/4706 l/h" (IFCTEXT)
    COBIE Water quantity 32 °C (6/12 °C) = "9285/9785 l/h" (IFCTEXT)
    COBIE Water quantity 32 °C (8/14 °C) = "7626/8126 l/h" (IFCTEXT)
    COBIE Weight = "172 kg" (IFCTEXT)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "TopVent_MC" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "8" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Type Name = "MC-9-D" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "MC-9-D" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 14.4032172035194 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 2.40810019602765 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    A = 1100. (IFCLENGTHMEASURE) [MILLI METRE]
    E = 594. (IFCLENGTHMEASURE) [MILLI METRE]
    E/2 = 297. (IFCLENGTHMEASURE) [MILLI METRE]
    F = 882. (IFCLENGTHMEASURE) [MILLI METRE]
    G = 940. (IFCLENGTHMEASURE) [MILLI METRE]
    H = 845. (IFCLENGTHMEASURE) [MILLI METRE]
    I = 935. (IFCLENGTHMEASURE) [MILLI METRE]
    J = 31.75 (IFCLENGTHMEASURE) [MILLI METRE]
    K = 1132. (IFCLENGTHMEASURE) [MILLI METRE]
    M = 31.75 (IFCLENGTHMEASURE) [MILLI METRE]
    O = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    P = 1050. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 2190. (IFCLENGTHMEASURE) [MILLI METRE]
    U = 1220. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Air flow direction visibility = FALSE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Hydronic Return,Hydronic Supply,Sanitary,Supply Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Air flow rate = "5000.0 m3/h" (IFCTEXT)
    Condensate quantity 28 °C (6/12 °C) = "0.0/0.1 kg/h" (IFCTEXT)
    Condensate quantity 28 °C (8/14 °C) = "0.0/0.0 kg/h" (IFCTEXT)
    Condensate quantity 32 °C (6/12 °C) = "25.6/31.2 kg/h" (IFCTEXT)
    Condensate quantity 32 °C (8/14 °C) = "15.7/21.3 kg/h" (IFCTEXT)
    Condensate quantity = "150.0 kg/h" (IFCTEXT)
    Heat output -5/-15 °C (60/40 °C) = "86.7/89.3 kW" (IFCTEXT)
    Heat output -5/-15 °C (80/60 °C) = "142.0/144.6 kW" (IFCTEXT)
    Maximum mounting height -5/-15 °C (60/40 °C) = "11.7/11.7 m" (IFCTEXT)
    Maximum mounting height -5/-15 °C (80/60 °C) = "9.3/9.4 m" (IFCTEXT)
    Octave sound power level - 1000 Hz = "75 dB" (IFCTEXT)
    Octave sound power level - 125 Hz = "67 dB" (IFCTEXT)
    Octave sound power level - 2000 Hz = "75 dB" (IFCTEXT)
    Octave sound power level - 250 Hz = "70 dB" (IFCTEXT)
    Octave sound power level - 4000 Hz = "74 dB" (IFCTEXT)
    Octave sound power level - 500 Hz = "73 dB" (IFCTEXT)
    Octave sound power level - 63 Hz = "49 dB" (IFCTEXT)
    Octave sound power level - 8000 Hz = "68 dB" (IFCTEXT)
    Relative humidity of the fresh air 28 °C (6/12 °C) = "40/60 %" (IFCTEXT)
    Relative humidity of the fresh air 32 °C (6/12 °C) = "40/60 %" (IFCTEXT)
    Sensible cooling capacity 28 °C (6/12 °C) = "38.1/37.7 kW" (IFCTEXT)
    Sensible cooling capacity 28 °C (8/14 °C) = "33.2/32.9 kW" (IFCTEXT)
    Sensible cooling capacity 32 °C (6/12 °C) = "47.4/47.1 kW" (IFCTEXT)
    Sensible cooling capacity 32 °C (8/14 °C) = "42.6/42.2 kW" (IFCTEXT)
    Sound pressure level (at a distance of 5 m) = "59 dB(A)" (IFCTEXT)
    Supply air temperature -5/-15 °C (60/40 °C) = "46.1/46.0 °C" (IFCTEXT)
    Supply air temperature -5/-15 °C (80/60 °C) = "64.4/64.2 °C" (IFCTEXT)
    Supply air temperature 28 °C (6/12 °C) = "11.8/12.0 kW" (IFCTEXT)
    Supply air temperature 28 °C (8/14 °C) = "13.4/13.6 °C" (IFCTEXT)
    Supply air temperature 32 °C (6/12 °C) = "12.7/12.9 kW" (IFCTEXT)
    Supply air temperature 32 °C (8/14 °C) = "14.3/14.5 °C" (IFCTEXT)
    Total cooling capacity 28 °C (6/12 °C) = "38.1/37.8 kW" (IFCTEXT)
    Total cooling capacity 28 °C (8/14 °C) = "33.2/32.9 kW" (IFCTEXT)
    Total cooling capacity 32 °C (6/12 °C) = "64.8/68.3 kW" (IFCTEXT)
    Total cooling capacity 32 °C (8/14 °C) = "53.3/56.7 kW" (IFCTEXT)
    Total sound power level = "81 dB(A)" (IFCTEXT)
    Water content of heating coil = "7.9 l" (IFCTEXT)
    Water pressure drop -5/-15 °C (60/40 °C) = "6/6 kPa" (IFCTEXT)
    Water pressure drop -5/-15 °C (80/60 °C) = "15/15 kPa" (IFCTEXT)
    Water pressure drop 28 °C (6/12 °C) = "13/13 kW" (IFCTEXT)
    Water pressure drop 28 °C (8/14 °C) = "10/10 kPa" (IFCTEXT)
    Water pressure drop 32 °C (6/12 °C) = "39/43 kW" (IFCTEXT)
    Water pressure drop 32 °C (8/14 °C) = "26/30 kPa" (IFCTEXT)
    Water quantity -5/-15 °C (60/40 °C) = "3725/3837 l/h" (IFCTEXT)
    Water quantity -5/-15 °C (80/60 °C) = "6101/6212 l/h" (IFCTEXT)
    Water quantity 28 °C (6/12 °C) = "5451/5409 l/h" (IFCTEXT)
    Water quantity 28 °C (8/14 °C) = "4756/4706 l/h" (IFCTEXT)
    Water quantity 32 °C (6/12 °C) = "9285/9785 l/h" (IFCTEXT)
    Water quantity 32 °C (8/14 °C) = "7626/8126 l/h" (IFCTEXT)
    Weight = "172 kg" (IFCTEXT)
  Electrical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Connected load = "3.6 kW" (IFCTEXT)
    Current consumption max. = "5.9A" (IFCTEXT)
    Frequency = "50 Hz" (IFCTEXT)
    Permitted voltage tolerance = "+/-5%" (IFCTEXT)
    Protection rating = "IP 54" (IFCTEXT)
    Series fuse = "13A" (IFCTEXT)
    Supply voltage = "3x400 V AC" (IFCTEXT)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Extract air temperature max. = "50°C" (IFCTEXT)
    Pressure of the heating medium max. = "800 kPa" (IFCTEXT)
    Supply air temperature max. = "60°C" (IFCTEXT)
    Temperature of the heating medium max. = "90°C" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Effective electric power input = "1.56 kW" (IFCTEXT)
    Floor area covered = 946. (IFCAREAMEASURE) [SQUARE_METRE]
    Nominal air flow rate = 2.5 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Static efficiency of the fans = "63.6%" (IFCTEXT)