IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-06-05T08:15:21"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_0715(x64) - Exporter 2015.0.2016.0512 - Default UI"
Application: "Autodesk Revit MEP 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit MEP 2015 (ENU)"

People and organizations
  Person "valentino.jugovic" of Organization (no name given)
  Owner history of Person "valentino.jugovic" of Organization (no name given) | application "Autodesk Revit MEP 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit MEP 2015 (ENU)" | change NOCHANGE | created 1559601733 (2019-06-03T22:42:13Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "THC-6-BC" | names: "TopVent_THC:THC-6-BC:938047" | material: materials ("HOVAL WHITE", "HOVAL RED") | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Graphics, Identity Data, Mechanical

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "TopVent_THC: THC-6-BC" (IFCLABEL)
    Family and Type = "TopVent_THC: THC-6-BC" (IFCLABEL)
    Type = "TopVent_THC: THC-6-BC" (IFCLABEL)
    Type Id = "TopVent_THC: THC-6-BC" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    COBIE Air flow rate = "3100 m3/h" (IFCTEXT)
    COBIE Condensate quantity 22 °C (50/70 %) - 6/12 °C = "0.0/13.5 kg/h" (IFCTEXT)
    COBIE Condensate quantity 22 °C (50/70 %) - 8/14 °C = "0.0/7.9 kg/h" (IFCTEXT)
    COBIE Condensate quantity 26 °C (50/70 %) - 6/12 °C = "8.6/30.2 kg/h" (IFCTEXT)
    COBIE Condensate quantity 26 °C (50/70 %) - 8/14 °C = "3.0/24.6 kg/h" (IFCTEXT)
    COBIE Condensate quantity = "90 kg/h" (IFCTEXT)
    COBIE Connected load = "3.6 kW" (IFCTEXT)
    COBIE Current consumption max. = "5.9A" (IFCTEXT)
    COBIE Effective electric power input = "0.76 kW" (IFCTEXT)
    COBIE Extract air temperature max. = "50°C" (IFCTEXT)
    COBIE Floor area covered = "537.0" (IFCTEXT)
    COBIE Frequency = "50 Hz" (IFCTEXT)
    COBIE Heat output 16/20 °C (60/40 °C) = "26.9/23.3 kW" (IFCTEXT)
    COBIE Heat output 16/20 °C (80/60 °C) = "47.0/43.4 kW" (IFCTEXT)
    COBIE Maximum mounting height 16/20 °C (60/40 °C) = "14.6/15.5 m" (IFCTEXT)
    COBIE Maximum mounting height 16/20 °C (80/60 °C) = "11.6/12.0 m" (IFCTEXT)
    COBIE Nominal air flow rate = "6000.0" (IFCTEXT)
    COBIE Octave sound power level - 1000 Hz = "71 dB" (IFCTEXT)
    COBIE Octave sound power level - 125 Hz = "59 dB" (IFCTEXT)
    COBIE Octave sound power level - 2000 Hz = "71 dB" (IFCTEXT)
    COBIE Octave sound power level - 250 Hz = "62 dB" (IFCTEXT)
    COBIE Octave sound power level - 4000 Hz = "67 dB" (IFCTEXT)
    COBIE Octave sound power level - 500 Hz = "68 dB" (IFCTEXT)
    COBIE Octave sound power level - 63 Hz = "41 dB" (IFCTEXT)
    COBIE Octave sound power level - 8000 Hz = "58 dB" (IFCTEXT)
    COBIE Permitted voltage tolerance = "+/-5%" (IFCTEXT)
    COBIE Pressure of the heating medium max. = "800 kPa" (IFCTEXT)
    COBIE Protection rating = "IP 54" (IFCTEXT)
    COBIE Sensible cooling capacity 22 °C (50/70 %) - 6/12 °C = "20.4/18.5 kW" (IFCTEXT)
    COBIE Sensible cooling capacity 22 °C (50/70 %) - 8/14 °C = "20.4/16.0 kW" (IFCTEXT)
    COBIE Sensible cooling capacity 26 °C (50/70 %) - 6/12 °C = "25.2/23.2 kW" (IFCTEXT)
    COBIE Sensible cooling capacity 26 °C (50/70 %) - 8/14 °C = "22.7/20.8 kW" (IFCTEXT)
    COBIE Series fuse = "13A" (IFCTEXT)
    COBIE Sound pressure level (at a distance of 5 m) = "54 dB(A)" (IFCTEXT)
    COBIE Static efficiency of the fans = "63.6%" (IFCTEXT)
    COBIE Supply air temperature 16/20 °C (60/40 °C) = "31.3/33.5 °C" (IFCTEXT)
    COBIE Supply air temperature 16/20 °C (80/60 °C) = "41.3/43.5 °C" (IFCTEXT)
    COBIE Supply air temperature 22 °C (50/70 %) - 6/12 °C = "13.9/14.9 °C" (IFCTEXT)
    COBIE Supply air temperature 22 °C (50/70 %) - 8/14 °C = "13.9/16.1 °C" (IFCTEXT)
    COBIE Supply air temperature 26 °C (50/70 %) - 6/12 °C = "15.5/16.5 °C" (IFCTEXT)
    COBIE Supply air temperature 26 °C (50/70 %) - 8/14 °C = "16.7/17.7 °C" (IFCTEXT)
    COBIE Supply air temperature max. = "60°C" (IFCTEXT)
    COBIE Supply voltage = "3x400 V AC" (IFCTEXT)
    COBIE Temperature of the heating medium max. = "90°C" (IFCTEXT)
    COBIE Total cooling capacity 22 °C (50/70 %) - 6/12 °C = "20.4/27.7 kW" (IFCTEXT)
    COBIE Total cooling capacity 22 °C (50/70 %) - 8/14 °C = "20.4/21.4 kW" (IFCTEXT)
    COBIE Total cooling capacity 26 °C (50/70 %) - 6/12 °C = "31.1/43.7 kW" (IFCTEXT)
    COBIE Total cooling capacity 26 °C (50/70 %) - 8/14 °C = "24.8/37.5 kW" (IFCTEXT)
    COBIE Total sound power level = "76 dB(A)" (IFCTEXT)
    COBIE Water content of cooling coil = "7.9 l" (IFCTEXT)
    COBIE Water content of heating coil = "4.6 l" (IFCTEXT)
    COBIE Water pressure drop 16/20 °C (60/40 °C) = "4/3 kPa" (IFCTEXT)
    COBIE Water pressure drop 16/20 °C (80/60 °C) = "13/11 kPa" (IFCTEXT)
    COBIE Water pressure drop 22 °C (50/70 %) - 6/12 °C = "15/28 kPa" (IFCTEXT)
    COBIE Water pressure drop 22 °C (50/70 %) - 8/14 °C = "15/17 kPa" (IFCTEXT)
    COBIE Water pressure drop 26 °C (50/70 %) - 6/12 °C = "36/71 kPa" (IFCTEXT)
    COBIE Water pressure drop 26 °C (50/70 %) - 8/14 °C = "23/52 kPa" (IFCTEXT)
    COBIE Water quantity 16/20 °C (60/40 °C) = "1157/1001 l/h" (IFCTEXT)
    COBIE Water quantity 16/20 °C (80/60 °C) = "2020/1864 l/h" (IFCTEXT)
    COBIE Water quantity 22 °C (50/70 %) - 6/12 °C = "2925/3960 l/h" (IFCTEXT)
    COBIE Water quantity 22 °C (50/70 %) - 8/14 °C = "2925/3064 l/h" (IFCTEXT)
    COBIE Water quantity 26 °C (50/70 %) - 6/12 °C = "4448/6263 l/h" (IFCTEXT)
    COBIE Water quantity 26 °C (50/70 %) - 8/14 °C = "3552/5367 l/h" (IFCTEXT)
    COBIE Weight = "248 kg" (IFCTEXT)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "TopVent_THC" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "11" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Type Name = "THC-6-BC" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "THC-6-BC" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 6.8578799029899 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.29000410392744 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    (X) = 1120. (IFCLENGTHMEASURE) [MILLI METRE]
    A = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    B = 1647. (IFCLENGTHMEASURE) [MILLI METRE]
    E = 594. (IFCLENGTHMEASURE) [MILLI METRE]
    E/2 = 297. (IFCLENGTHMEASURE) [MILLI METRE]
    F = 758. (IFCLENGTHMEASURE) [MILLI METRE]
    G = 101. (IFCLENGTHMEASURE) [MILLI METRE]
    H = 179. (IFCLENGTHMEASURE) [MILLI METRE]
    I = 349. (IFCLENGTHMEASURE) [MILLI METRE]
    J = 427. (IFCLENGTHMEASURE) [MILLI METRE]
    K = 760. (IFCLENGTHMEASURE) [MILLI METRE]
    N = 1030. (IFCLENGTHMEASURE) [MILLI METRE]
    O = 792. (IFCLENGTHMEASURE) [MILLI METRE]
    P = 312. (IFCLENGTHMEASURE) [MILLI METRE]
    Q = 31.75 (IFCLENGTHMEASURE) [MILLI METRE]
    R = 31.75 (IFCLENGTHMEASURE) [MILLI METRE]
    S = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Air flow direction visibility = FALSE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Hydronic Supply,Hydronic Return,Sanitary,Hydronic Supply" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Condensate quantity 22 °C (50/70 %) - 6/12 °C = "0.0/13.5 kg/h" (IFCTEXT)
    Condensate quantity 22 °C (50/70 %) - 8/14 °C = "0.0/7.9 kg/h" (IFCTEXT)
    Condensate quantity 26 °C (50/70 %) - 6/12 °C = "8.6/30.2 kg/h" (IFCTEXT)
    Condensate quantity 26 °C (50/70 %) - 8/14 °C = "3.0/24.6 kg/h" (IFCTEXT)
    Heat output 16/20 °C (60/40 °C) = "26.9/23.3 kW" (IFCTEXT)
    Heat output 16/20 °C (80/60 °C) = "47.0/43.4 kW" (IFCTEXT)
    Maximum mounting height 16/20 °C (60/40 °C) = "14.6/15.5 m" (IFCTEXT)
    Maximum mounting height 16/20 °C (80/60 °C) = "11.6/12.0 m" (IFCTEXT)
    Octave sound power level - 1000 Hz = "71 dB" (IFCTEXT)
    Octave sound power level - 125 Hz = "59 dB" (IFCTEXT)
    Octave sound power level - 2000 Hz = "71 dB" (IFCTEXT)
    Octave sound power level - 250 Hz = "62 dB" (IFCTEXT)
    Octave sound power level - 4000 Hz = "67 dB" (IFCTEXT)
    Octave sound power level - 500 Hz = "68 dB" (IFCTEXT)
    Octave sound power level - 63 Hz = "41 dB" (IFCTEXT)
    Octave sound power level - 8000 Hz = "58 dB" (IFCTEXT)
    Sensible cooling capacity 22 °C (50/70 %) - 6/12 °C = "20.4/18.5 kW" (IFCTEXT)
    Sensible cooling capacity 22 °C (50/70 %) - 8/14 °C = "20.4/16.0 kW" (IFCTEXT)
    Sensible cooling capacity 26 °C (50/70 %) - 6/12 °C = "25.2/23.2 kW" (IFCTEXT)
    Sensible cooling capacity 26 °C (50/70 %) - 8/14 °C = "22.7/20.8 kW" (IFCTEXT)
    Sound pressure level (at a distance of 5 m) = "54 dB(A)" (IFCTEXT)
    Supply air temperature 16/20 °C (60/40 °C) = "31.3/33.5 °C" (IFCTEXT)
    Supply air temperature 16/20 °C (80/60 °C) = "41.3/43.5 °C" (IFCTEXT)
    Supply air temperature 22 °C (50/70 %) - 6/12 °C = "13.9/14.9 °C" (IFCTEXT)
    Supply air temperature 22 °C (50/70 %) - 8/14 °C = "13.9/16.1 °C" (IFCTEXT)
    Supply air temperature 26 °C (50/70 %) - 6/12 °C = "15.5/16.5 °C" (IFCTEXT)
    Supply air temperature 26 °C (50/70 %) - 8/14 °C = "16.7/17.7 °C" (IFCTEXT)
    Total cooling capacity 22 °C (50/70 %) - 6/12 °C = "20.4/27.7 kW" (IFCTEXT)
    Total cooling capacity 22 °C (50/70 %) - 8/14 °C = "20.4/21.4 kW" (IFCTEXT)
    Total cooling capacity 26 °C (50/70 %) - 6/12 °C = "31.1/43.7 kW" (IFCTEXT)
    Total cooling capacity 26 °C (50/70 %) - 8/14 °C = "24.8/37.5 kW" (IFCTEXT)
    Total sound power level = "76 dB(A)" (IFCTEXT)
    Water content of cooling coil = "7.9 l" (IFCTEXT)
    Water content of heating coil = "4.6 l" (IFCTEXT)
    Water pressure drop 16/20 °C (60/40 °C) = "4/3 kPa" (IFCTEXT)
    Water pressure drop 16/20 °C (80/60 °C) = "13/11 kPa" (IFCTEXT)
    Water pressure drop 22 °C (50/70 %) - 6/12 °C = "15/28 kPa" (IFCTEXT)
    Water pressure drop 22 °C (50/70 %) - 8/14 °C = "15/17 kPa" (IFCTEXT)
    Water pressure drop 26 °C (50/70 %) - 6/12 °C = "36/71 kPa" (IFCTEXT)
    Water pressure drop 26 °C (50/70 %) - 8/14 °C = "23/52 kPa" (IFCTEXT)
    Water quantity 16/20 °C (60/40 °C) = "1157/1001 l/h" (IFCTEXT)
    Water quantity 16/20 °C (80/60 °C) = "2020/1864 l/h" (IFCTEXT)
    Water quantity 22 °C (50/70 %) - 6/12 °C = "2925/3960 l/h" (IFCTEXT)
    Water quantity 22 °C (50/70 %) - 8/14 °C = "2925/3064 l/h" (IFCTEXT)
    Water quantity 26 °C (50/70 %) - 6/12 °C = "4448/6263 l/h" (IFCTEXT)
    Water quantity 26 °C (50/70 %) - 8/14 °C = "3552/5367 l/h" (IFCTEXT)
    Weight = "248 kg" (IFCTEXT)
  Electrical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Connected load = "3.6 kW" (IFCTEXT)
    Current consumption max. = "5.9A" (IFCTEXT)
    Frequency = "50 Hz" (IFCTEXT)
    Permitted voltage tolerance = "+/-5%" (IFCTEXT)
    Protection rating = "IP 54" (IFCTEXT)
    Series fuse = "13A" (IFCTEXT)
    Supply voltage = "3x400 V AC" (IFCTEXT)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Air flow rate = "3100 m3/h" (IFCTEXT)
    Condensate quantity = "90 kg/h" (IFCTEXT)
    Extract air temperature max. = "50°C" (IFCTEXT)
    Pressure of the heating medium max. = "800 kPa" (IFCTEXT)
    Supply air temperature max. = "60°C" (IFCTEXT)
    Temperature of the heating medium max. = "90°C" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Effective electric power input = "0.76 kW" (IFCTEXT)
    Floor area covered = 537. (IFCAREAMEASURE) [SQUARE_METRE]
    Nominal air flow rate = 1.66666666666667 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Static efficiency of the fans = "63.6%" (IFCTEXT)