IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2022-06-24T15:55:04"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1656078904 (2022-06-24T13:55:04Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_RPI-FSNE-2-6_LOD400:RPI - 4.0 FSN4E" | object type "BC_Hitachi_RPI-FSNE-2-6_LOD400:RPI - 4.0 FSN4E" | names: "BC_Hitachi_RPI-FSNE-2-6_LOD400:RPI - 4.0 FSN4E:3785" | material: materials ("Operation and service space", "<Unnamed>") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Dimensions

Types
  IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_RPI-FSNE-2-6_LOD400:RPI - 4.0 FSN4E" | 1 occurrence | material: "Operation and service space" | property sets: Constraints, Construction, Data, Dimensions, Electrical, Electrical Engineering

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "BC_Hitachi_RPI-FSNE-2-6_LOD400: RPI - 4.0 FSN4E" (IFCLABEL)
    Family and Type = "BC_Hitachi_RPI-FSNE-2-6_LOD400: RPI - 4.0 FSN4E" (IFCLABEL)
    Type = "BC_Hitachi_RPI-FSNE-2-6_LOD400: RPI - 4.0 FSN4E" (IFCLABEL)
    Type Id = "BC_Hitachi_RPI-FSNE-2-6_LOD400: RPI - 4.0 FSN4E" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "BC_Hitachi_RPI-FSNE-2-6_LOD400" (IFCTEXT)
    MasterFormat = "23 73 00" (IFCTEXT)
    Omniclass = "23-33 25 00" (IFCTEXT)
    Refrigerant = "R410A" (IFCTEXT)
    Uniformat = "D3040" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RPI - 4.0 FSN4E" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "HITACHI" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RPI - 4.0 FSN4E" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 8.30225580931309 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.6726605824636 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Air outlet distance = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance from left Drain pipe = 254. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance from left liquid pipe = 92. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance from left pipe = 92. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain pipe Height = 113. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Gas pipe Height = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    Input Height = 195. (IFCLENGTHMEASURE) [MILLI METRE]
    Input Width = 1240. (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Diameter = 9.52 (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid pipe Height = 86. (IFCLENGTHMEASURE) [MILLI METRE]
    Operation and Service pipe distance = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Outlet Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Output Height = 176. (IFCLENGTHMEASURE) [MILLI METRE]
    Output Width = 1257. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Depth = 275. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 1474. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "32019" (IFCTEXT)
    BC_OBJECT_ID = "9326" (IFCTEXT)
    BC_OBJECT_VERSION = "#1" (IFCTEXT)
    BC_VARIANT_ID = "29782" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Standard Duct units . Possibility to reduced the capacity" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Manufacturer = "HITACHI" (IFCTEXT)
    Model = "Ducted unit RPI-FSN3/4 - 2 to 6" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Product Code = "7E424020" (IFCTEXT)
    Reference = "RPI - 4.0 FSN4E" (IFCTEXT)
    Type Comments = "RPI - 4.0 FSN4E" (IFCTEXT)
    Type Name = "RPI - 4.0 FSN4E" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Sanitary,Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Air flow Speed (high/medium/low) m3/min) = "30/28/25" (IFCTEXT)
    Classification = "None" (IFCIDENTIFIER)
    External static pressure = 45. (IFCPRESSUREMEASURE) [PASCAL]
    Fan motor type (output) = 250. (IFCPOWERMEASURE) [WATT]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Operation and Service space = TRUE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Gross Weight = 0. (IFCMASSMEASURE) [KILO GRAM]
  Data | properties | on 1 type object
    Acoustic Pressure Level Maxi (dB) = 30. (IFCREAL)
    Acoustic Pressure Level Medium (dB) = 28. (IFCREAL)
    Acoustic Pressure Level Mini (dB) = 25. (IFCREAL)
    Floor Number = "" (IFCTEXT)
    Installation Instructions = "" (IFCTEXT)
    Local Number = "" (IFCTEXT)
    Mass = 48. (IFCMASSMEASURE) [KILO GRAM]
    Network Name = "" (IFCTEXT)
    Sound power max (dB(A)) = 30. (IFCREAL)
  Electrical | properties | on 1 type object
    AC Current Max = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    AC Max Power = 0. (IFCPOWERMEASURE) [WATT]
    AC Nominal Power = 0. (IFCPOWERMEASURE) [WATT]
    Absorbed power at nominal conditions = 0. (IFCPOWERMEASURE) [WATT]
    Active power of use = 0. (IFCPOWERMEASURE) [WATT]
    Actual load output phase 1 = 0. (IFCPOWERMEASURE) [WATT]
    Actual load output phase 2 = 0. (IFCPOWERMEASURE) [WATT]
    Actual load output phase 3 = 0. (IFCPOWERMEASURE) [WATT]
    Angular Displacement = "" (IFCTEXT)
    Battery Charging Circuit Rated Voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Battery Current = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Breaker Size = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Busbar Trunkings = FALSE (IFCBOOLEAN)
    Cooling Capacity Rated = 0. (IFCPOWERMEASURE) [WATT]
    Core Diameter = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cos φ = 0. (IFCREAL)
    Coupling = "" (IFCTEXT)
    Current Rating = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Current max DC = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Effective rated output = 250000. (IFCPOWERMEASURE) [WATT]
    Nominal Current = 5. (IFCELECTRICCURRENTMEASURE) [AMPERE]
  Electrical Engineering | properties | on 1 type object
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Maximum AC Voltage = 253. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Minimum AC Voltage = 207. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Poles = "1" (IFCTEXT)
    Usage Current = 5. (IFCELECTRICCURRENTMEASURE) [AMPERE]
  Energy Analysis | properties | on 1 type object
    Cooling Capacity = 11200. (IFCPOWERMEASURE) [WATT]
    Heating Capacity = 12500. (IFCPOWERMEASURE) [WATT]
  Materials and Finishes | properties | on 1 type object
    Color = "" (IFCTEXT)
  Mechanical - Flow | properties | on 1 type object
    AHU Dual Deck = FALSE (IFCBOOLEAN)
    Capacity = 0. (IFCPOWERMEASURE) [WATT]
    Exhaust Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Filter class = "" (IFCTEXT)
    Maximum Air Flow = 500. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Maximum Air Pressure = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Minimum Air Flow = 416.666666666667 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    New air pressure = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Plumbing | properties | on 1 type object
    Hot water flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]