IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "ExchangeRequirement []"
Time stamp: "2023-01-31T10:41:43"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "22.0.2.392 - Exporter 22.0.2.392 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "dev2NW3Q" of Organization (no name given)
  Owner history of Person "dev2NW3Q" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1675158102 (2023-01-31T09:41:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_RAS-4-6FS(V)NME_LOD400:RAS-6FSNME" | object type "BC_Hitachi_RAS-4-6FS(V)NME_LOD400:RAS-6FSNME" | names: "BC_Hitachi_RAS-4-6FS(V)NME_LOD400:RAS-6FSNME:5564" | material: materials ("<Unnamed>", "Service space walls in 4 directions") | property sets: Pset_BuildingElementProxyCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints

Types
  IFCBUILDINGELEMENTPROXYTYPE "BC_Hitachi_RAS-4-6FS(V)NME_LOD400:RAS-6FSNME" | 1 occurrence | material: materials ("<Unnamed>", "Service space walls in 4 directions") | property sets: Constraints, Construction, Data, Dimensions, Electrical, Electrical Engineering

Property sets
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "BC_Hitachi_RAS-4-6FS(V)NME_LOD400: RAS-6FSNME" (IFCLABEL)
    Family and Type = "BC_Hitachi_RAS-4-6FS(V)NME_LOD400: RAS-6FSNME" (IFCLABEL)
    Type = "BC_Hitachi_RAS-4-6FS(V)NME_LOD400: RAS-6FSNME" (IFCLABEL)
    Type Id = "BC_Hitachi_RAS-4-6FS(V)NME_LOD400: RAS-6FSNME" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Cooling Capacity = 16000. (IFCPOWERMEASURE) [WATT]
    Family Name = "BC_Hitachi_RAS-4-6FS(V)NME_LOD400" (IFCTEXT)
    Heating Capacity = 18000. (IFCPOWERMEASURE) [WATT]
    Refrigerant Type = "R410" (IFCTEXT)
    Refrigerant charge before shipment = 4.1 (IFCMASSMEASURE) [KILO GRAM]
    Sound level = 70. (IFCREAL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RAS-6FSNME" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Color = "Natural Grey (1.0Y8.5/0.5)" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RAS-6FSNME" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 8.43599404453058 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 2.53027829479786 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Gas Diameter = 15.88 (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Diameter = 9.52 (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Depth = 370. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 1380. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Packing dimensions (H x W x D) = "1515 mm x 1012 mm x 460 mm" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BC_MODEL_ID = "167059" (IFCTEXT)
    BC_OBJECT_ID = "29707" (IFCTEXT)
    BC_OBJECT_VERSION = "#4" (IFCTEXT)
    BC_VARIANT_ID = "193051" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Designation = "RAS-6FSNME" (IFCTEXT)
    GTIN (Global Trade Item Number) = "" (IFCTEXT)
    Manufacturer = "Hitachi Air Conditioning Europe SAS" (IFCTEXT)
    Model = "Set Free Mini - RAS-4-6 FS(V)NME" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Product Code = "" (IFCTEXT)
    Reference = "RAS-6FSNME" (IFCTEXT)
    Type Comments = "RAS-6FSNME" (IFCTEXT)
    Type Name = "RAS-6FSNME" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Power,Undefined,Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
    Motor power = 3660. (IFCPOWERMEASURE) [WATT]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Service space = TRUE (IFCBOOLEAN)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Construction | properties | on 1 type object
    Compressor Model = "ATH420" (IFCTEXT)
    Compressor Quantity = 1 (IFCINTEGER)
    Compressor Type = "SHEC Rotary" (IFCTEXT)
    Gross Weight = 129. (IFCMASSMEASURE) [KILO GRAM]
    Net Weight = 119. (IFCMASSMEASURE) [KILO GRAM]
  Data | properties | on 1 type object
    Approximate Packing Volume = 0.71 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Condenser Fan Quantity = 2 (IFCINTEGER)
    Condenser Fan Type = "Axial" (IFCTEXT)
    Flow Control = "Micro-Computer control expansion valve" (IFCTEXT)
    Heat Exchanger = "Multi Pass Cross - Finned Tube" (IFCTEXT)
    Refrigeration Oil Charge = "1.65 L/Unit" (IFCTEXT)
    Refrigeration Oil Type = "α 68HES-H" (IFCTEXT)
    Sound Pressure Level (night mode) = "53 (48)" (IFCTEXT)
  Electrical | properties | on 1 type object
    Motor - Number of Poles = 4 (IFCINTEGER)
  Electrical Engineering | properties | on 1 type object
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Nominal Voltage = 400. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Number of Poles = 3. (IFCREAL)
  Materials and Finishes | properties | on 1 type object
    Color = "Natural Grey (1.0Y8.5/0.5)" (IFCTEXT)
  Mechanical - Flow | properties | on 1 type object
    Nominal Air Flow = 2416.66666666667 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Nominal Static Pressure = 30. (IFCPRESSUREMEASURE) [PASCAL]